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Description automatically generated]PRODUCTION SPECS

1. IMAGE CAPTURE REQUIREMENTSa. RESOLUTION REQUIREMENTSRESOLUTION: 	Preferably 5K or greater (UHD minimum upon approval)

FORMAT:	RAW
Minimum of 16-bit Linear or 10-bit Log processing
	Maximum Compression: 1:6

FRAME RATE:	23.98 

ASPECT RATIO 
FOR PRIMARY 
DELIVERY: 	16:9

GAMMA: 	Wide Gamut 2.4 Preferred

LENS: 	Spherical 

b. CAMERAS
APPROVED FOR USE
Red Cameras with 4K or greater resolution (preferably the Dragon)
	Maximum Compression 1:4
Canon C300
Alexa Mini LF
Alexa LF
Panavision DXL2
Sony Venice
Alexa 35

REQUIRING FES APPROVAL
Canon C500
Black Magic Ursa/Ursa mini 

NOT ALLOWED
Sony F7 
Alexa Mini 
Black Magic Pocket 4K
Sony FS7
Sony FX6


2. QUALITY CONTROL CONSIDERATIONS DURING PRODUCTIONPlease watch for and avoid the following production issues. They often require costly fixes to pass quality control for delivery of the picture: 1. Avoid Logos & Branding2. Watch for booms/production equipment/crew in frame or in reflections (mirrors, car windows or sides, etc.)3. Tape/Markers on the floor etc. 4. Lens glare5. Iris Shifts6. Equipment Shadows in frame3. RAW FOOTAGE BACK UPProduction should create (3) redundant copies of all RAW media created on set (Picture and Sound). The (3) copies should be stored in separate locations. Shuttle drives should be utilized to get one copy to the Post Production Facility on a daily/weekly basis (depending on practical needs determined by Post Supervisor).
4. ADDITIONAL FOOTAGE
All additional media used in the film (i.e. Stock Footage, VFX, Archival) must be UHD or greater, 16:9 23.98, unless approved by FES.

STOCK FOOTAGE must be UHD or greater, 16:9 23.98 for Commercial Use

NOTE: SHOTS UPLOADED ONTO STOCK FOOTAGE WEBSITES MAY HAVE BEEN RECORDED AT A DIFFERENT FRAME RATE THAN THE FILE AVAILABLE FOR DOWNLOAD. SUCH FOOTAGE MAY BE 23.98 FPS BUT WILL STUTTER OR HAVE MOIRE/ALIASING ISSUES AND NOT PASS QUALITY CONTROL. IT IS THE PRODUCER’S RESPONSIBILITY TO CONFIRM STOCK FOOTAGE PLAYS BACK SMOOTHLY AT 23.98 FPS PRIOR TO DELIVERY. 

5. DAILIES (if required)
On Projects requiring dailies, Producer is expected to upload proxy (H.264) versions of the shot footage with a LUT approximating the desired finished color grade, and sync audio for FES review. Each day should be provided as a single stringout with TC window burn and clip names. FES will provide access to frame.io or similar for distribution of dailies. Each day’s footage should be available for review within 24 hours after completion of that day’s production.
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